Questions and answers:

Question: Please Confirm LTO 8 SAS or FC  
Please confirm HBA requirements – HBA requirements will be based on the exact model of the existing HPE Proliant Server – Please confirm.

Answer: 1/8 G2 or above Tape Autoloaders should be able to connect the server externally.